Our company offers on sale plane AN-74 which is in our property.
AN-74 – The easy transport multi-purpose plane, is intended for operation on airlines of average extent. Reliability of the plane proves to be true an operational experience of various updatings in all climatic zones from–60 With to + 45 With and in the conditions of high mountains. The given type of the plane has especially well proved, being maintained in the countries of Africa, and in particular in Angola. Two engines 6500 кgf everyone, highly mechanised  a wing allow to carry out the truncated launch-landing and flights with abrupt trajectories that is very important at work in high-mountainous TAKE-OFF - LANDING STRIP the limited sizes. The chassis of high passableness and engines highly located over the earth allow to maintain the plane on damp, wet, snow-covered LANDING STRIP with a soil, cespitose and ice covering. Repeated reservation of the basic systems, high manoeuvrability, both in flight, and on the earth, favourably distinguish planes AN-74 at operation in extreme situations and difficult tactical conditions. Universality of plane AN-74 has use more potential.
Interior of a transport cabin of plane An-74 
The Transport cabin of An-74 has the dimensions optimised in the sizes of the basic stream of transported cargoes, and allows to transport cargoes in containers and packaged on rigid pallets, non-standard (bales, flanks, etc.) cargoes, and also not self-propelled and self-propelled wheel technics (cars of type " Jeep -S47" and another.) The Aperture of the cargo hatch is closed by a stage which can be lowered on the earth and to use as a gangway, or to shift forward under a fuselage that provides convenience of loading of the plane directly from a car body. Loading and unloading of the cargoes packaged on pallets. Cargoes in containers and other it is made by means of the onboard loading device by load-carrying capacity 2500 kgf (24.5 кН). Loading and unloading of self-propelled technics is made under the own steam, and not self-propelled wheel technics - by means of the tractor and the loading device.

	
1. A barrier wall 

2. Soft mobile a partition

3. A place of the second илота 

4. A place of the flight mechanic 

5. A toilet 

6. Clothes 

7. The Workplace of a hydrobroad gull of the second class 

8. The Berth 

9. The container with cargo 

10. A place of the commander of an aircraft 

11. The Workplace of the navigator 

12. A door-gangway 

13. Buffet 

14. The Workplace of the radio operator 

15. The Workplace of a hydrobroad gull of the first class


	1. Барьерная стенка 

2. Мягкая движная перегородка

3. Место второго илота

4. Место бортмеханика

5. Туалет

6. Гардероб

7. Рабочее место гидролога второго класса

8. Спальное место

9. Контейнер с грузом

10. Место командира воздушного судна

11. Рабочее место штурмана

12. Дверь-трап

13. Буфет

14. Рабочее место радиста

15. Рабочее место гидролога первого класса 


	AIRCRAFT IDENTIFICATION AN-74

	Date of manufactory
	25.03.1992 y. ХГАПП.

	Specified Life H/Y
	20 000 hour., 20 years (Term lasts to 40 000 h. And 40 years, the general appointed resource

	Capitally a recovery work (CHECK)
	will be executed in 2009

	OPERATED AFTER THE LAST CRW
	0 h

	Total airframe hours/land
	3017/1200 


Operating since new: 3017 hours, 1200 settlements 
Extreme flight 31.05.2005

20.09.2001 In Ivanovo is executed II stage Capitally a recovery work (CHECK)  at an operating time 2945 hours, 1089 settlements . By the decision 06.401-74-2004 a target date of service of 13 years (10 000 hour, 5000 settlements) 
	

                  AIRFRAME MAINTENANCE PROGRAMME

	Aircraft Maintenance Program Provided by:
	Manufacturer, based on maintenance regulation

	Repair Station Providing Service:
	АРЗ-412, Kiev

	Primary Line Maintenance Provided by:
	Operator


Engine Type and Model D-36, ser.3
	
	Date of Manufacture
	Number of overhaul
	       Date OH, y
	Total Flight 
Hours/ cycle
	After OH, h

	Engine R
708036112А055
	27.03.1991 y.
	1
	2006
	3060/1318    
	0


	Engine L
708036112А061
	30.06.1991 y.
	1
	2006
	3063/1321
	0

	Engine Manufacturer:
	Мотор Сич

	
            
    ENGINE MAINTENANCE PROGRAMME

	Engine Aircraft Maintenance Program Provided by
	Manufacturer, based on maintenance regulation

	Engine Oil Type
	ВНИИНП-50-1-4У


Both of the engine are modified for a possibility of use of a EXTREME MODE  Also resources 3600 hours/2400 of cycles, service life till November, 01, 2007. 

The appointed resource 8000 hours, 5334 cycles
APU ТА-12 # 13012007 Engine Manufacturer: “Гидравлика” Уфа
	Life limit between Contrl Regenerative Check

	Date of Manufacture
	Resources h/ Cycles /y
	Total Flight Hours/starts

	01.09.91 г.
	500 /1500 /20
	328 /1365

	
            
    ENGINE MAINTENANCE PROGRAMME

	Engine Aircraft Maintenance Program Provided by
	Manufacturer, based on maintenance regulation

	Engine Oil Type
	ВНИИНП-50-1-4У


Further increase: Specified Life: 

Frame 40 000 Hrs, 20 000 landings, 30 years 

Left engine 8 000 Hrs, 7 273 cycles, 18 years 

Right engine 8 000 Hrs, 7 273 cycles, 18 years 

Max take-off weight 34,8

Max payload 10000 kgs 

Length 28.07 m 

Wing span 31.89 m 

Height 8.75 m 

Cruising speed 550 km/hr 

Maximum speed 700 km/hr 

Flight altitude 11.600 km 

Dimensions of cargo compartment (bxhxl) 9.5 x 2.15 x 2.2 

Cargo door size 2.4 x 2.27 m 

Volume of cargo compartment 45-50 m3 

Engine two turbofan engines D-36 3A series, chapter III compliant

Cost "AS IS" with above-stated Technical characteristics - $ 3000000.00 US dollars. 
We have reduced the price to $ 2000000.00 US dollars.  Without TCAS, EGPWS, BRNAV


The plane is in good repair. After idle time at factory the plane demands prolongation. 
Our company will execute forms on prolongation of a glider, engines and units. 
After prolongation the plane will have a resource before repair and the certificate of the flight validity - 2 years. 
After performance of all prolongations the plane has the permission to fly 6 years. 
After 6 years forms again are required. 
Rough term of performance of the given works - 2 month. 

PRICE in full flight readiness - reduced to $ 3,5 M US FOR ACCELERATION OF PURCHASE. 
And TCAS, EGPWS, BRNAV will be installed.
The plane will be painted on request of the Buyer for a payment of the Buyer.
At desire of the Buyer our company has possibility to convert the plane in a cargo-passenger or convertible variant. 

We can make the fine and comfortable the VIP salon which has been already equipped by other plane. A salon photo in an attachment. Re-equipment cost roughly + 2 000 000-00 US dollars – IT IS THE PRICE OF FACTORY OF THE MANUFACTURER. 

Delivery term – 6 months.
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