COMMERCIAL OFFER.
1. Type of aircraft 


An-74-200
The AN-74-200 operates with combined cargo and passenger configurations, making it an attractive option for customers wishing to send cargo with cargo attendants. The airplane is complies with all modern aviation standards, including stage 3 noise certification. The airplane is equipped with a back cargo ramp that allows facilitating loading procedures. argo transportation up to 7.500 kg; transportation of vehicles and wheeled equipment, cargo on pallets and bulk cargo.
Cargo is carried on special pallets or as bulk cargo. With the airborne cargo handling device automatically controlled by operator, rolling and winch equipment ensures easy cargo loading and unloading, drive in/out of vehicles process. Besides the An-74-200 features the unique capability of rear ramp retracting under the fuselage allowing to minimize further loading and unloading time.
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Number of aircraft 1 
Number of crew members 4-6 
Number of passenger seats 10 
Max take-off weight 36,5 
Max payload 7.500 kgs 
Length 28.07 m 
Wing span 31.89 m 
Height 8.75 m 
Cruising speed 550 km/hr 
Maximum speed 700 km/hr 
Flight altitude 10.100 km 
Flight range 
Load 1.5 T - 4.150 km 
Load 5 T - 2.800 km 
Load 7.5 T - 2.150km 
Dimensions of cargo compartment (bxhxl) 9.5 x 2.15 x 2.2 
Cargo door size 2.4 x 2.27 m 
Volume of cargo compartment 45-50 m3 
Engine two turbofan engines D-36 3A series, chapter III compliant

TECHNICAL  DATA.

1. Date of manufactory: 

Serial Nr.

Date of manufactory

AN-74-200 - 10.06.1994
Left engine (Lotarev D-36 serial 3A)

708036423A024
25.02.1993
Right engine (Lotarev D-36 serial 3A)
708036133A001
22.02.1993

Auxiliary Power Unit TA-12


32012019

14.07.1993
2. The following equipment are installed and approved on this aircraft:
· Magnetic compass 



KI-13 (1 unit)

· Heading System 



BSFK-1 (1 unit)

· Autopilot  




SAU-72-03 (1 unit)

· Radar  





BURAN-74 (1 unit)

· Radio airborne (118,000-136,975 MHz) VHF BAKLAN-20D1 8.33 KHz, FM immunity (2 units)

· Radio airborne (2,000-23,9999 KHz) HF
JADRO (1 unit)

· Emergency Radio Station (121,5 MHz)
R-855 (2 units)

· Navigation system (VOR and ILS)

KURS-МP-70 FM immunity (2 units)

· Navigation system (DME)


SD-75 (2 units)

· Transponder (A,C mode)


SO-72 (1 unit)

· Modes S Transponder Level 4 (A, C mode)
XS-950 (1 unit)

· Flight data recorder



BUR-2-3 (1 unit) and K3-63 (1 unit)

· Cockpit voice recorder


MARS-BM (1 unit) 

· Ground Proximity Warning System

SPPZ-1-3 (1 unit)

· Radio Altimeters



A-037D1 (2 units)

· Airborne Collision Avoidance System
TCAS-2000 (1 unit)

· B-RNAV




MALVA-4 (1 unit)

NVS-74 (1 unit)

· EGPWS




MARK VIII

· ELT





Kannod-406
· GPS





KLN-90B

3. Damages history, overloads and other special conditions while in service – Nil
4. Specified Life:

Frame  


40 000 Hrs, 
20 000 landings,
30 years
Left engine

8 000 Hrs, 
7 273 cycles,

18 yeras

Right engine

8 000 Hrs, 
7 273 cycles,

18 yeras

AU TA-12


500 Hrs,
1.000 start up,

10 years

5. Life until firts overhaul:

Frame


3 600 Hrs
1 800 landings

Left engine
 
3 000 Hrs, 
2 000 cycles

Right engine 

3 000 Hrs, 
2 000 cycles

APU TA-12

500 Hrs, 
1 000 start up

6. Date of last overhaul:

Frame


3.08.2007 (КВР-2)
Left engine 

Nil

Right engine

Nil

APU TA-12

Nil




7. Operating since new:

Frame


1.125 Hrs, 
670 landings

Left engine 

1.167 Hrs, 
665 cycles

Right engine 

1.167 Hrs, 
665 cycles

APU TA-12

156 Hrs, 
813 start up

8. Remain overhaul period:

 Frame


3.600 Hrs, 
1 800 landings
  
  Calendar time 
untill 02.08.2011
 Left engine

1.833 Hrs, 
1 335 cycles

 Calendar time 
01.03.2008

 Right engine 

1.833 Hrs, 
1 335 cycles

   Calendar time 
01.03.2008

 APU TA-12 

344 Hrs, 
187 start up

 Calendar 


untill 11.02.2008

9. Life till next check:

Frame


300±30 Hrs or 4months±15 days
10. Presence of the operational documentation - is present.
We are pleased offer for sale cargo airplane AN-74-200 in perfect conditions.

Asking price is 5.200.000 US READY FOR FLIGHT.

The Buyer will give the Letter on interest and will confirm readiness to buy the plane for a suggested price. Lets out LOI for a suggested price and will approve, that the Buyer is ready to expose the deposit of 5 % before survey of the plane and not later than within 10 days from date of the LOI. Conditional deposition should be in the Europe. 
The plane will be removed from the market for the coordinated period for survey and signings of the contract. 

Payment only 100 % an advance payment under the contract.

