	GENERAL  DATA OF THE  AIRKRAFT   IL-76TD                
	   DATA ON  ENGINES  D-30KP2
	 Normal
	Available

	                                    01.10.2010
	
	ENGINE’ 1   
	
	

	Date of Manufacture
	31.05.1986
	         Date of Manufacture 25.03.1986.
	
	

	Life Limit  (Hours/ Years)
	30 000 / 30
	 Life limit  (Hours)
	9 000
	12 000

	Life Limit (Landings)
	8000
	 Life limit  (Cycles)
	
	

	Total Hours Since New
	          16 000
	Life Limit Between Overhaul (Hours)
	
	

	Total Landings Since New
	          4850
	Life Limit Between Overhaul (Cycles)
	
	

	Life Limit Between Overhaul (Hrs/Yrs)
	5000 / 5-20 on TC 
	Life Limit Between Overhaul (Years)
	
	

	Life Limit Between Overhaul (Landings)
	 5000
	Total Hours Since New
	
	

	Total Hours Since Last Overhaul
	
	Total Cycles Since New
	
	

	Total Landings Since Last Overhaul
	
	Total Hours Since Last Overhaul
	      
	

	Date of Last Overhaul
	15.07.1991
	Total Cycles Since Last Overhaul
	     
	

	Number of Overhaul
	1
	Date of Last Overhaul
	
	

	WEIGHT DATA (Kg)
	
	Number of Overhaul
	
	

	Certified Taxi Weight
	194 000
	
	
	

	Certified Take Off Weight
	193 000
	ENGINE’ 2   
	
	

	Certified Maximum Landing Weight
	151 500
	        Date of Manufacture 29.10.1983
	
	

	Certified Maximum Zero Fuel Weight
	140 700
	Life limit  (Hours)
	9 000
	12 000

	Fuel Capacity
	87 000
	Life limit  (Cycles)
	
	

	AVIONICS
	
	Life Limit Between Overhaul (Hours)
	
	

	VHF COM SYS` 1 (8,33)
	Baklan-20
	Life Limit Between Overhaul (Cycles)
	
	

	VHF COM SYS` 2 (8,33)
	Baklan-20
	Life Limit Between Overhaul (Years)
	
	

	HF COM SYS
	Yadro
	Total Hours Since New
	
	

	VHF NAV SYS` 1
	Kurs MP-2
	Total Cycles Since New
	
	

	VHF NAV SYS` 2
	Kurs MP-2
	Total Hours Since Last Overhaul
	      
	

	ADF NAV SYS` 1
	ARK-15M
	Total Cycles Since Last Overhaul
	
	

	ADF NAV SYS` 2
	ARK-15M
	Date of Last Overhaul
	
	

	WEATHER RADAR
	+
	Number of Overhaul
	
	

	LOW RANGE RADIO ALTIMETER` 1
	RW-5M
	
	
	

	LOW RANGE RADIO ALTIMETER` 2
	RW-5M
	ENGINE’ 3   
	
	

	FDR
	MSRP-64 M5
	     Date of Manufacture  31.07.1995
	
	

	CVR
	+
	Life limit  (Hours)
	9 000
	12 000

	ATC TRANSPONDER
	SO-70
	Life limit  (Cycles)
	3 375
	4 620

	CABIN INTERPONE SYS
	+
	Life Limit Between Overhaul (Hours)
	4 780
	6 000

	AUTOPILOT
	SAU-1T-2BТ
	Life Limit Between Overhaul (Cycles)
	1 540
	1540

	EMERGENCY HF COM SYS
	+
	Life Limit Between Overhaul (Years)
	6
	16

	EMERGENCY VHF COM SYS
	R-855UM
	Total Hours Since New
	8 783
	

	DME
	+
	Total Cycles Since New
	
	

	ALTIMETER (FEET)` 1
	WMF-50K
	Total Hours Since Last Overhaul
	650
	

	ALTIMETER (FEET)` 2
	WMF-50K
	Total Cycles Since Last Overhaul
	
	

	GPS receiver
	KLN 90B
	Date of Last Overhaul
	12.07.06
	

	TCAS
	TCAS-II
	
	
	

	
	
	Number of Overhaul
	2
	

	   APU                              Model
	ТА-6А
	
	
	

	Serial number
	
	ENGINE’ 4     
	
	

	Date of Manufacture / Overhaul 
	26.10.93/ 26.11.01
	     Date of  Manufacture 02.03.1980
	
	

	Date of Installation
	
	
	
	

	Life limit  (Hours)
	3200
	Life limit  (Hours)
	9 000
	12 000

	Life limit  (Cycles)
	5 000
	Life limit  (Cycles)
	
	

	Hours Since New
	
	Life Limit Between Overhaul (Hours)
	
	

	Cycles Since New
	
	Life Limit Between Overhaul (Cycles)
	
	

	Total     Hours   Since Last Overhaul
	
	Life Limit Between Overhaul (Years)
	
	

	ADDITIONAL EQUIPMENT
	
	Total Hours Since New
	
	

	TCAS, BRNAV, ELT, RVSM 
	+
	Total Cycles Since New
	
	

	EGPWS
	+
	Total Hours Since Last Overhaul
	
	

	ТТА, TDS
	+
	Total Cycles Since Last Overhaul
	
	

	
	
	Date of Last Overhaul
	
	

	
	
	Number of Overhaul
	
	

	Life limits and life times of the airframe are settled accor- ding to the Decision of the Design Bureau “Ilyushin” and  Russian DCA № 5.9-60ГA date issued 15.02.06)

Calendar TBO will be extended for 1 years
	Available designated life limits 

Available life limits between OH based on Decision  № 207/006-127/99 (3.30KP.1.2.(3)-05/24)


Remainder of the resources:

Life Limit  (Hours/ landings/Years) –    14 000/ 3150 / 30.05.2016

	FUSELAGE AND CARGO HOLD

	Cargo cabin dimensions

	     Length (including ramp)
	M
	24.54

	     Length (exluding ramp)
	M
	20.00

	     Width
	M
	3.40

	     Height
	M
	3.46

	Cargo door dimensions
	mm
	3,400 x 3,450

	Usable Volume
	m³
	185

	 


	MASS CHARACTERISTICS


	Maximum takeoff mass

	Kg

	190,000


	Maximum landing mass

	Kg

	151,000


	Maximum mass of paid loading *

	Kg

	45,000


	Basic operating mass

	Kg

	92,500


	Mass of empty plane

	Kg

	88,000


	Maximum fuel reserve

	Kg

	42,500


	 


	PERFORMANCE


	Cruise speed

	Km/h

	800


	Maximum range with maximum payload

	Km

	3,650


	Maximum practical range

	Km

	4,500


	Range with half of payload

	M

	7,300


	Advantageous altitude

	M

	9,000


	Service ceiling with all engines operating

	M

	12,000


	Takeoff run length

	M

	1,700


	Landing run length

	M

	1,200


	Aviation fuel consumption in the cruise regimen *

	Tons/h

	8.6


	 


	ENGINES


	Type

	D-30KP


	Engine thrust

	kgf/kWt

	4 x 12,000



	


Price  on condition FCA 
2 x 1986 IL-76TD, the price of  $1,5M US for each without the VAT (the PRICE WITHOUT ENGINES).

Engines can be established with a resource from 30 % to 100 % (we have after the repair, two available short time) and the price from $325 000 to $500 000 for each accordingly without the VAT.
All planes have the equipment: TCAS, BRNAV, ELT, RVSM, EGPWS + 
TTA, TDS +
Conditions of sale:

Preliminary specification. The final specification will be given after receipt of the Preliminary Letter of intent. This Letter of Intent must specify the name of the end user and the signature.

Simultaneously with a preliminary letter of intent buyer sends POF worth at least 3.5 million dollars (the approximate amount of the Contract). After receiving proposals and specifications and if the buyer agrees to price and condition of the aircraft, the Buyer is to provide a letter of interest and confirm commitment to fly the aircraft on the proposed price, confirm that the buyer is ready to put a deposit of 5% before inspecting the aircraft no later than 10 days from the date of his LOI. Escrow should be in Europe or by agreement. Perhaps the signing of the Contract for e-mai and the payment of mortgage or prepayment from the buyer to back up aircraft. The aircraft will be withdrawn from the market for an agreed period for inspection and purchase contract. Payment - only 100% advance payment on the contract.

Other conditions are not acceptable.
ПРЕДВАРИТЕЛЬНАЯ СПЕЦИФИКАЦИЯ 1986 Ил-76ТД.

Более подробные данные по двигателям и ВСУ после получении Предварительного Письма о намерении от Покупателя и Конечного пользователя.
а) Планер ИЛ-76 ТД (по состоянию 01.10.2010г.)
Дата выпуска                                    31.05.1986

Дата КВР                                          15.07.1991

Назначенный срок службы             30 лет

Назначенный ресурс, час/пос.        30 000/ 8 000 

Наработка СНЭ, час/пос.                16 000 /4850
Наработка ППР, час/пос.                10 000 /3150

Остаток назнач. ср. сл.                    30.05.2016г.

Остаток межрем.ср. сл.                   

Остаток назнач. ресурса, час/пос.  
Остаток межрем. ресурса, час/пос.  

б) Авиадвигатели:  Д-30КП-2
                                                      №1                 №2                  №3                  №4

2 X 1986 Ил-76ТД, цена каждого - 1,5 млн. долларов без НДС (ЦЕНА БЕЗ ДВИГАТЕЛЕЙ).

Двигатели могут быть установлены с ресурсом от 30% до 100% (после ремонта, два в наличии) и цена от 325 000$ до 500 000$ соответственно без НДС.
в) Вспомогательная силовая установка ТА-6А:

г) Перечень оборудования установленного на ИЛ-76ТД:

	№ п/п
	Наименование  оборудования
	Кол-во. (шт)

	1.
	Радиолокационная станция  КП2В-5
	1

	2.
	Радиолокационная станция  КП3А
	             1

	3.
	Инерциальная система И-11-76
	1

	4.
	Управляющий вычислительный комплекс КП1Д-76-5
	1

	5.
	Самолетный ответчик СО-70
	1

	6.
	Самолетный ответчик СОМ-64
	1

	7.
	Спутниковая навигационная система KLN-90В
	1

	8.
	Система предупреждения столкновения в воздухе TCAS-II
	1

	9.
	Система автоматического управления САУ-1Т-2БТ
	1

	10.
	Радиосистема ближней навигации и посадки РСБН—7С
	1

	11.
	Аппаратура навигации и посадки КУРС-МП2
	1

	12.
	Самолетный дальномер СДК-67А
	1

	13.
	Автоматический радиокомпас АРК-15М
	2

	14..
	Радиовысотомер РВ-5М
	2

	15.
	Доплеровский измеритель ДИСС-013
	1

	16.
	Система воздушных сигналов СВС1-72-1В
	2

	17.
	Точная курсовая система ТКС-П
	1

	
	Высотомер ВБЭ-2А
	2

	18.
	Футомер ВМФ-50К
	2

	19.
	СРПБЗ: ТТА-12S со встроенным приёмоизмерителем СНС производства ЗАО «ТРАНЗАС»;

МФИ: ТDS-56D с функцией рельефа местности
	1

	20.
	УКВ р/с «Баклан-20Д»
	2

	21.
	КВ р/с «Ядро»
	2

	22.
	МСРП-64М-5
	1

	23.
	К3-63
	1

	24.
	Изд. «020»
	1

	25.
	Р-855УМ
	1

	26.
	АРМ-406П, 

АРМ-406АС1
	1

1

	27
	Оборудование для полетов по RWSM
	1


Условия продажи:

Спецификация может быть предоставлена после получения Предварительного Письма о намерении от Покупателя с указанием Конечного пользователя. Одновременно с Предварительным Письмом о намерении Покупатель присылает POF на сумму не менее 3,5 миллионов долларов (примерная сумма Контракта). После получения Покупателем предложения и согласия с ценой и состоянием самолета, Покупатель предоставит Письмо о заинтересованности и подтвердит готовность покупать самолет по предложенной цене, подтвердит, что Покупатель готов выставить депозит 5% перед осмотром самолета не позднее, чем в течение 10 дней от даты своего LOI. Условное депонирование должно быть в Европе или по согласованию. Возможно подписание Контракта по e-mai и оплата залога Покупателем для резервирования самолета. Самолет будет снят с рынка на согласованный период для осмотра и подписания контракта покупки. Оплата - только 100% предоплата по контракту. 

Другие условия не приемлемы.
Specifications subject to verification upon inspection and aircraft is subject to prior sale or withdrawal from the market

